#!/bin/bash

echo "IMPORTANT TASKS

Buildroot

[1] init Buildroot (min config)

[2] exec Buildroot menu

[3] build firmware with buildroot

[4] copy sdcard.img > ~/shared

Debootstrap

[5] build firmware with debootstrap

[6] copy sdcard.img > ~/shared

Other

[E] end

Your choice:"

read nr

if [[ $nr != [0-9]\* ]]; then

echo "end"

elif [ $nr -eq 1 ]; then

echo "init Buildroot (min config)"

cd ~/buildroot

make BR2\_EXTERNAL=../custom O=../make dhbw\_minimal\_defconfig

cd ..

elif [ $nr -eq 2 ]; then

echo "exec Buildroot menu"

cd ~/make

make menuconfig

cd ..

elif [ $nr -eq 3 ]; then

echo "build firmware with buildroot"

cd ~/make/

make

cd ..

elif [ $nr -eq 4 ]; then

echo "copy sdcard.img > ~/shared"

cp ~/make/images/sdcard.img ~/shared/

elif [ $nr -eq 5 ]; then

echo "build firmware with debootstrap"

~/db-build.sh

elif [ $nr -eq 6 ]; then

echo "copy sdcard.img > ~/shared"

cp ~/out/debian/sdcard.img ~/shared/

else

echo "end"

fi